To properly run this software, you must first make a new directory on your hard drive, we

suggest the following path, C:/D-2Inc/VCAL-1.04. Then all the files in this directory should be copied to

the new directory. At that point, you can double-click on the executable file (VCal.exe) and the program

should run. Please read all the instructions on the opening screen and have a working knowledge of the

JF-1A-HH sensor before actually trying to calibrate the unit.

Questions and comments can be directed to D-2 Inc., 508-329-2046