To properly run this software, you must first make a new directory on your hard drive, we

suggest the following path, C:/D-2Inc/StickCAL-1\_30. Then all the files from this compressed (zip) file should be copied to the new directory. At that point, you can double-click on the executable file (StickCal.exe) and the program should run. The optimal screen resolution for this program is 1920 x 1080 with a 100% scale factor.

Please read all the instructions on the opening screen and have a working knowledge of the JF-1A-ST sensor before actually trying to calibrate the unit.

Questions and comments can be directed to D-2 Inc., 508-329-2046